On 10th July 2017 are opened public consultations regarding the HOPS's proposal for thresholds of types B, C and D of power-generating modules in accordance with COMMISSION REGULATION (EU) 2016/631, Article 5(3):

<https://www.hops.hr/en/connection-network-codes>

Comments can be delivered on e-mail address: javno.savjetovanje@hops.hr

Deadline for submission of comments on the proposed thresholds is 21th August, 2017.

Tablica 2. Suggested threshold for production modules type A, B, C and D

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|   | Typ A | Typ B | Typ C | Typ D |
| Voltage | < 110 kV | < 110 kV | < 110 kV | ≥110 kVor |
| Rated Power | 0,8 kW ≤ tip A < 500 kW | 500 kW≤ tip B < 5 MW | 5 MW≤ tip C < 10 MW | < 110 kVi10 MW ≤ tip D |