|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Categories of PGMs (PPMs)** | **Limit**  | **Subcategories** | **New limit** | **Specific requirements** *of the NC RfG* |
| **A** | 800 W | **A1** | **≥ 800 W; <11 kW** | *According to article. 13*  |
| **A2** | **≥ 11 kW; <100 kW** | *According to article. 13, article 14.2, 14.3, 14.4, 14.5 and article 20 for PPMs* |
| **B** | 1 MW | **B1** | **≥ 100 kW; <1 MW** | *According to article 14, article 17 and article 20 for PPMs* |
| **B2** | **≥ 1 MW; <30 MW** | *According to article 14, article 17,and article 15.2, 15.3, 15.4, 15.5a, 15.5b, 15.5c, 15.6a, 15.6b, 15.6c , article 18 and article 21 for PPMs* |
| **C** | 50 MW | **C** | **≥ 30 MW** | *According to article 15, article 18 and article 21 for PPMs* |
| **D** | 75 MW | **D** | **≥ 75 MW** | *According to article 16, article19 and čl.22 for PPMs* |